| CY8CKIT-062S2-43012 BSP

Peripheral Default BSP Settings

Resource | Parameter | Value | Remarks
--- | --- | --- | ---
ADC | VREF | 1.2 V |
Measurement type | Single Ended |
Input voltage range | 0 to 2.4 V (0 to 2*VREF) |
Output range | 0x000 to 0x7FF |
DAC | Reference source | VDDA |
Input range | 0x000 to 0xFFF |
Output range | 0 to VDDA |
Output type | Unbuffered output |
I2C | Role | Master | Configurable to slave mode through HAL function
Data rate | 100 kbps | Configurable through HAL function
Drive mode of SCL & SDA pins | Open Drain (drives low) | External pull-up resistors are required
LpTimer | Uses WCO (32.768 kHz) as clock source & MCWDT as counter; 1 count = 1/32768 second or 32768 counts = 1 second
SPI | Data rate | 100 kpbs | Configurable through HAL function
Slave select polarity | Active low |
UART | Flow control | No flow control | Configurable through HAL function
Data format | 8N1 | Configurable through HAL function
Baud rate | 115200 | Configurable through HAL function

© Cypress Semiconductor Corporation, 2019-2022.